PHOTOGRAPHY WORKSHOPS

TOYO OPERATION

Setting Up

- attach to tripod

- loosen rear tilt screws (big knobs)

- open from bottom

- tighten rear tilt screws

- unlock front tilt

- unlock front rise

- pull forward

- lock front rise (with red dot visible)

- lock front tilt

- move lens plane to front standard

- attach lens

- view screen (rotate if necessary)

- focus (loupe)

- calculate exposure compensation for bellows extension

 ½ focal length = 1 stop / 1 focal length = 2 stop

- attach cable release

- set aperture / shutter speed (taking into account exposure compensation)

- close lens (but make sure shutter isn’t cocked)

- load film back

- insert film back

- cock shutter

- remove dark slide

- take picture

- turn dark slide around (black side) and put back

Putting Away

- unlock front rise

- unlock front tilt

- fold down

- move lens bed back

- unlock rear tilt

- fold up

- lock rear tilt